4 in 1 Auto Focus Camera OSD Instruction
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Know the OSD cable and control it

UP&Down the button

Left&Right the button

Press Down the button

Zoom in &Zoom out the Lens

UP  the button = Zoom in

Down the button =Zoom out

Don’t too be fast or constantly. Up&down steps by steps,let the lens have time to focus and zoom . 

If can’t focus well , then left&right the button gently.

OSD menu

Press down the button. Then the main Menu should be come out in the screen .

Up&Down button choose the item after setting press down the button and saved it .

Reset: Choose the item 10 Reset the Camera and save it.
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Signal switch

Choose the item 2. Right the button 3 times (1,2,3) then press down confirm it .

Choose the Signal and Apply it

[image: image2.png]MAIN MENU

1. LENS MANUAL
3. BACKLIGHT OFF
4. WHITE BAL ATW
5. DAY&NIGHT EXT
6. NR o

7. SPECIAL o

8. ADJUST oI

9. AF d

10. EXIT SAVE&END



                    [image: image3.png]HIDDEN

1.MONITOROUT ~ AHD |
2. ADC TEST. OFF
3. AE TEST OFF
4. FIRMWARE d

5. RETURN RET




PAL&NTSC

Press down the button 5 Seconds . It will switch
